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! Please read the manual before installing and using this lighting
Keep it for future reference              



Thank you for purchasing our device.
We make every effort to ensure the best quality of our products and to meet your expectations.

If you have any remarks or comments, please share them with us.

We will be grateful for any suggestions that will help us make products that are even better and devices that satisfy your needs.


R&D Team
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[bookmark: _Toc494321520]Statement
The product is good packing when ship out the factory. All users should strictly abide by the warnings and instructions stated in this manual, any damage and results due to misuse and the neglect of this operating manual will be excluded from the deal responsibility this manual will not informed in additionally if have technical changes.

1. [bookmark: _Toc494321521]Production introduces
[bookmark: _Toc494321522]Thank you for choosing this product. This is our latest development of intelligent, efficient products, beautiful and fluent, combined with the advanced technology of the stage lighting today. It has advanced international electronic control technology and excellent human nature chemical industry. The product is fully in conformity with the CE standard and the recipient country. The standard DMX512 signal mode is supported by the RDM protocol.
Production enforce standard IEC 60598-1:2014，IEC60598-2-17:2017.

Channels mode:  16/24CH; 
Lamp: 470W White LED Engine ;
Life time：20000 hours;
Light Source Luminous Flux：30000；
power: AC110-240V,50/60Hz;
Total power: 700W;
Display: 2.8 inch  screen display, can reverse 180°;
Color wheel:  7 fix colors+white+CMY+CTO.CT:2800-5600K
Fixed gobo :   8 gobo + white.
Rotation gobo:  6 gobo+ white, changeable;
Prism:  4 facet prism ,Frost function;
Beam angel : 6～42°;
Dimmer : 0-100% linear adjustment ;
Iris: Disphragm adjustable
Cut: 4 plates. Aftercut,the pattern can rotation 180°
connector can set dmx address with power and upgrade the software.
Position lock system: Magnetism position lock system
Pan : 540°;  8Bit/16Bit ;
Tilt :  270°;  8Bit/16Bit ;
IP Rate: IP20;

2. Fixture size

Product size：404（L）×306（W）×736（H）mm
[image: ]
3. [bookmark: _Toc494321523]Part introduction
01 — Lens
02 — Body
03 — Arm
04 — Tilt Lock
05 — Pan Lock
06 — Light base
07 — Handle
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The structure of each part of the product is marked, and the main components of the lamps and lanterns are made up of the product names, so as to further understand the lamps and lanterns products.01 —Control panel
02 — USB Port
03 — Button
01 — DMX In
02 — DMX Out 
03 — Power switch
04 — Power in
05 — Fuse
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The function of the product panel is introduced, the name of the part on the panel is indicated, and the functions and functions of each part are familiar.
4. A description of a color wheel, a GOBO wheel, and so on
Color wheel:  7 fix color +white+CMY+CTO. CT:2800-5600K
[image: ][image: ]

Fixed GOBO : 8 GOBO + white.Rich design, with the four prism better effect;
[image: ]
Rotation GOBO: 6 GOBO+ white.The rotation of the GOBO is smooth and the changeable is convenient.
[image: ]
Equipped with a four prism, positive and negative rotation; linear atomization function;The prism with  focused, rotated, enlarged and jitter, and the rotation speed can be adjusted.
5. Safety information
Safety warning:
This product is only suitable for professional use, and does not apply to security for other purposes.
After you got the lights, please check the package whether have any damage caused by transportation. If there is any damage, do not use this fixture, and please contact the dealer or manufacturer as soon as possible. This product is only suitable for indoor, IP20 protection class. Lamps should be kept dry to avoid Moisture, overheating or dusty environment. Prevent lamps meet water or any other liquid. The use of this product should pay attention to: fire, heat, electric shock, ultraviolet radiation, the lamp to explode or shedding caused serious or fatal injury.  Need to read the instructions before use energized or installing.  Follow through the operation of security methods and pay attention to the warning signs on the specification and equipment. If you have any problem for how to safely operate the equipment. Please contact your dealer. 
1.1. [image: u=2407575218,2844988952&fm=51&gp=0]Anti-high temperature
ta =40°C
Please don’t use the equipment if the temperature above 40℃[image: IIPZ@`4S_J0@(_~`0[LW@(0]
1.2. Burst prevention
The lens should be changed if had damaged or any problems. 
Don’t change the non-original manufacturer lens. Len size: ￠119mm×23mm
[image: u=61216684,2290708108&fm=15&gp=0]
1.3. To prevent falling wounding

Please don’t move the package by one person only.
When Hang the fixture, please must verify that the facilities to be able to   withstand the weight of the lamps at least 10 times more.
Please make sure the Mounting hardware is strong enough no any damage, and insurance for the safety rope as auxiliary security fixed in other facilities will need to verify before installation. Installing or removing the equipment, to make the pulley below the work location

1.4. UV protection and the bulb explosion

Prohibit straight viewpoint with exposed bulbs to avoid UV damage to the eyes;
Do not use the equipment without the lens screen and the lid;
The lens and the light head covers should be timely replaced if any damage to rupture
The Fixture should be used with the protection screen together.
[image: u=924525614,113233066&fm=52&gp=0]
1.5. Prevention of electric shock

The electrical connection must only be carried out with corresponding qualifications;
Before installing, make sure you use the power voltage lamps must comply with the identified power, voltage and have an overload or leakage protection;
[image: u=1164620996,2780990407&fm=52&gp=0]Each lamp must be properly grounded, installed in accordance with the relevant standards;
[image: }9T)4$84~_K49[FFU41SC@R]Cut off the power when stall or replace the lamp and the fuse;
Prohibit the use of a lightning storm or wet environment.
[image: d9abb482aa491d1f059f48412cb8b219]
1.6. To prevent burning or fire 
· The fixture can be mounted directly on the surface of ordinary combustible material.[image: ]
· Do not short-circuit temperature protection switch or fuse, use the specified type of fuse.
· The equipment must be installed away from inflammable and explosive materials.
· [image: ]The equipment should be projected range of 3 meters away objects and projectiles temperature less than 60 ° C;
· [image: u=484631801,3617214356&fm=23&gp=0]Fan or ventilation, at least in the range of 0.5 meters cannot be an obstacle.
· Do not place any object on the lens.
· Handling at least allow the device to cool for 20 minutes.
· Do not replace the non-original parts.

2. [bookmark: _Toc494321525]Package
2.1. Attachment
HOT BEAM 2R packed with fly-case of one in one, two in one, or carton box. Attach follow accessory.
ACCESSORY
	CONTENT
	QUANTITY

	USER MANUL
	      1 piece

	CLAMP (option)
	      2 pcs

	SIGNAL CABLE
	      1 piece



2.2. Transport protect lock
To protect the light, there is a protect lock; During the transport, the lock will have closed    keeping the item in safety state.

2.3. About pack stage
  1. Before packed, make sure power is off, and wait for at least 20mins for cooling down.
2. Before cleaning the fixture, make sure X, Y axis protect lock closed.
[image: 2D8[M2J@TPP0E~X8SFJ)JPS]3. After packed by plastic bag, high-lift the fixture with two handles besides the product. put the product into the fly-case up-side-down. 
4. After packed the product, put the accessory into the accessory case, then closed and lock the fly-case.
5. Fly-case only up stacked two layers. Prohibited upside down
6. When packed with carton box, equipment should be put into the foam first, then set into a carton, pay attention to the vertical position.

2.4. Unpacking
[bookmark: OLE_LINK8]Note: Before unpacking check the damage is whether due to the transportation or not, if you find any such damage, please do not use this item, and contact with the dealer or manufacturer as soon as possible.
· Open the fly-case, and discover the inside plastic bag.
· High-lift the product by two handles beside the bottom base and move it out.
· Before power on, make sure you have opened the X, Y axis lock!
3. [bookmark: _Toc494321526]Install standard
3.1. Install lock
HOT BEAM 2R can be placed on the stage, or mounted in an arbitrary direction of the truss. Two fast locks system could fix the item easily.

3.2. Equipment fixed
· Before installation must verify the fast lock is keep in good state, and can withstand at least 10 times the weight of product. Verify that the building can withstand at least 10 times of the total weight of the product and accessory equipment’s.
· Fix the hang fixture into the hole, which located on the base of the price. 
· Seize handle of fasteners, clockwise rotate 1/4 turn and lock. Installed other one fastener
· in the same method. 
· Using the safety cable which can withstand 10 times the weight of the equipment.
· [bookmark: OLE_LINK20][bookmark: OLE_LINK21][bookmark: OLE_LINK22][bookmark: OLE_LINK23][image: d9abb482aa491d1f059f48412cb8b219]Make sure the X, Y protect locks are opened, verify that within 3 meters there is no combustibles.

WARNING
Fixture must use two fixing devices, and make sure the fixing device have locked! And only fully clockwise rotate 90 ° can lock the hang fixture! Do remember plus a safety rope, and do not connect the safety rope to plastic handle. It should be connected to the hole on the base!

3.3. Fixture connects

[image: d9abb482aa491d1f059f48412cb8b219] Attention! One product only can accept one input one output.
HOT BEAM 2R DMX cable include 3 contact pins: 
Pin 1, FOR GROUND; Pin 2 connected to the negative polarity signal; The pin 3 connected to the positive polarity signal.

[bookmark: OLE_LINK7][bookmark: OLE_LINK9]DMX512 cable must use the professional shielded twisted pair cable; standard loudspeaker cable is not reliable to control the long-range data. 24AWG cable is suitable for more than 300 meters long-distance signal transmission and must add\ DMX 512 signal amplifier.
Do not use two outputs to separate the connection, if separate a continuous connection to branch, DMX512 splitter is necessary.
If use the DMX512 splitter. At first connect DMX512 Splitter input terminal to controller, and then connected from the splitter output terminal to next device.
[image: 11111][image: 222]Do as above guide to connect other device, and finally coupled with terminal insertion as following:





4. [bookmark: _Toc494321527]Power supply
4.1. Voltage, power, fuse specification

	Input Voltage
	Total Power
	Frequency

	
110~240V
	
150 W
	
50/60HZ



4.2. Power protect
[bookmark: OLE_LINK18][bookmark: OLE_LINK19]The equipment must be operated by professionals; Make sure that the voltage of power supply must be comply with the voltage identified on the lamp, and must have an overload or leakage electrical protection.
ATTENTION! 

[image: d9abb482aa491d1f059f48412cb8b219]Factory has equipped the standard 3 pin plug socket. Connect the power supply as below table.
If lamp cable is damaged, replacement should be operated by factory or qualified staff. Any question, please contact professionals or talk to a qualified electrician.

	[bookmark: OLE_LINK3]Live wire(L)
	Null(N)
	Ground wire
	[image: P0AAI1FW$12S[23{]`6U_8O]

	RED
	BLUE
	Yellow +Green
	


5. [bookmark: _Toc494321528]Lamp
5.1. Lamp description

	LAMP MODEL
	POWER OF LAMP
	LIFE/HOUR
	COLOR TEMPERATURE

	OSRAM SIRIUS HRI
	150 W
	4000 HOURS
	9300K



[image: d9abb482aa491d1f059f48412cb8b219]WARNING! 
There is a safety hazard or damage if install similar bulb to reduce the risk of damage to light, do change the lamp before using time over 90% of lamp life.


5.2. Lamp replace
[bookmark: OLE_LINK30][bookmark: OLE_LINK31][image: u=484631801,3617214356&fm=23&gp=0]Attention! When replace the lamp is forbidden to touch lamp with bare hand, to avoid the greasy dirt stains filament. filament must be kept clean. Disconnect the power. Before replace lamp, fixture need 20 minutes for lamp cooling. Fasten the head with Y axis protect lock in 60 ° position.
1. Use cross screwdriver to open the light body cover

2. After open the cover, you can see the lamp inside, please wait the lamp be cool after used but not touch it in hot status.









3. One hand press the lamp holder, another hand hold the lamp and pull out the wires








4. after take apart the lamp, please check the inside glasses, clear it will make the light better effect







5. installed the lamp after replaced.
6. [bookmark: _Toc494321529]Color wheel, gobo wheel
[image: ]

[image: ]Fixed Gobo






[image: ]Rotation Gobo

MINIHOT BEAM Have 6 linear prism and 8 facet prism. With Focus . Rotation . Zoom . Shaking . Rotation speed changeable
7. [bookmark: _Toc494321530]Control	panel
Display
Control wheel


Display: to display all information of fixture. 
Control wheel: can turn right, left and enter.
turn left  ： date	increase
turn right  ：date	decrease
Press function	：enter

8. [bookmark: _Toc494321531]CONTROL PANEL MENU OPERATE

	Main Menu
	Submenu 1
	Submenu 2
	Function SET
	Function description

	DMX Address
	
	
	001-512
	DMX Address number set

	











Display
	
"ShowReve"
	
	"Natu"
	Normal

	
	
	
	"Revl"
	reverse 180°

	
	
"Language"
	
	"Chin"
	Chinese 中文

	
	
	
	"English"
	English

	
	"BrigSett"
	
	000-255
	Brightness set

	
	

"Backligh"
	
	

"60S "
	Backlight close after delay
60S

	
	
	
	"Ligh"
	Backlight light always

	
	

MenuBack"
	
	

90S
	Menu back to mainmenu
after delay 90S

	
	
	
	"Off "
	Menu back not automatic

	
	


Backflah
	
	

open
	Backlight blinking when no
dmx

	
	
	
	

off
	Backlight not blinking when
no dmx

	
	"Return	"
	
	▲
	return

	


"Feature "
	


"XY Setup"
	"Xreverse"
	"Off "
	PAN SCAN Normal

	
	
	
	"Open"
	Pan Scan Reverse

	
	
	
"Yreverse"
	"Off "
	Tilt Scan normal

	
	
	
	"Open"
	Tilt Scan Reverse

	
	
	"XY Speed"
	"Fast"
	PAN/TILT FAST

	
	
	
	
	SPEED

	
	
	
	

"NORM"
	PAN/TILT NORMAL

	
	
	
	"Solw"
	PAN/TILT SLOW

	
	
	

"X	Angle"
	"360 ", "360 "
	Pan Angle 360°

	
	
	
	"540 ", "540 "
	Pan Angel 540°

	
	
	
	"630 ", "630 "
	Pan Angel 630°

	
	
	

"XY Fback"
	

"Off "
	PAN/TILT optical sensor testing off

	
	
	
	

"Open"
	PAN/TILT optical sensor testing on

	
	
	Return
	▲
	Return

	
	
"Shortcut"
	
	

"Off "
	Shortcust off for colors and gobos

	
	
	
	

"Open"
	Shortcust open for colors and gobos

	
	"FullColr"
	
	"Off "
	half color function

	
	
	
	"Open"
	full color function

	
	

"ChanMode"
	
	

"Smal"
	

Simplify mode

	
	
	
	"Stan"
	Standard mode

	
	"ReceMode"
	
	"DMX "
	Accept DMX

	
	
	
	"Wire"
	Accept Wireless

	
	
	
	"Auto"
	AutoRun

	
	
"RunMode "
	
	

"Slve"
	Accept other signal control

	
	
	
	"Musc"
	Sound active

	
	
	
	

"Auto"
	Inside program Run automatically

	
	"SigClear"
	
	"Off "
	keep signal data

	
	
	
	"Open"
	clear signal data

	
	DMX Reset
	
	Off
	Dmx reset not accept

	
	
	
	Open
	Dmx reset accept

	
	Return
	
	▲
	Return

	






"LampSett"
	

"Default "
	
	"Wink"
	Lamp off

	
	
	
	"Ilum"
	Lamp on

	
	

"Control "
	
	"Wink"
	Lamp off by manual

	
	
	
	"Ilum"
	lamp on by manual

	
	




"DmxLamp "
	
	

"Off "
	Close other signal control the lamp

	
	
	
	

"Open"
	Open other signal control the lamp

	
	
	
	0000-9999
	Lamp used time recorded

	
	"LampTime"
	
	
	

	
	

"ClearTim"
	
	★
	Password input Enter

	
	
	
	"Ilum"
	Clear Lamp time

	
	

"LampStat"
	
	"Wink"
	Lamp off

	
	
	
	"Ilum"
	Lamp on

	
	Return
	
	▲
	Return

	






"InfoSee "
	"WorkHour
"
	
	

0000-9999
	working hours memo for connect power

	
	"Times
"
	
	

0000-9999
	

Open times memo

	
	"Fan1Rota"
	
	0000-9999
	Fan rotation speed 1

	
	"Fan2Rota"
	
	0000-9999
	Fan rotation speed 2

	
	"Version "
	
	XMOA
	Version

	
	Spare time
	
	No limit
	No limit time

	
	Spare cut
	
	No limit
	No limit times

	
	Return
	
	▲
	Return

	
"Control "
	
	
	Chan 00-Chan
40
	

Control the Channels

	


















"AssiTool"
	"Factory "
	
	★
	Password input Enter

	
	
	
	"Fold"
	Recover Factory set

	
	
	
	"Save"
	Save factory set

	
	"Defaults"
	
	★
	Password input Enter

	
	
	
	"Fold"
	Recover to default

	
	Redress
	
	★
	Password input enter

	
	
	
	Reset01-10
	Set the motors

	
	

Chdefine
	
	Color wheel
Rotation 001
	Channels set by define

	
	
	
	

000……040
	Channels set by define

	
	"Brightne"
	
	★
	Password input Enter

	
	
	

"TimeLimi"
	

0000-9999
	Open fixture time limit

	
	
	"TimsLimi"
	0000-9999
	fixture times limit

	
	
	

TimeCLEA
	

clear
	Clear the time of used

	
	
	

CutClea
	

clear
	Clear the times of used

	
	
	"Passwor1"
	000-255
	Revise password 1

	
	
	"Passwor2"
	000-255
	Revise password 2

	
	
	"Passwor3"
	000-255
	Revise password 3

	
	
	"Passwor4"
	000-255
	Revise password 4

	
	
	"X Drivin"
	000-255
	pan main drive gear

	
	
	"X Driven"
	000-255
	Pan slave drive gear

	
	
	"Y Drivin"
	000-255
	Tilt main drive gear

	
	
	"Y Driven"
	000-255
	Tilt slave drive gear

	
	
	
	
	

	
	
	"LampPowe"
	"Off "
	Ballast earthed

	
	
	
	"total 5V", "Open"
	

Ballast 5V

	
	
	

"YAngle	"
	

000-255
	Tilt angel rotation set

	
	
	"Return	"
	000-255
	return

	
	

"Checksum
"
	

01-10"
	
	


Check Cabrilate data

	
	Return
	
	▲
	Return

	CHANLEVE
	
	
	Chan1..140
	Show the dmx address

	
MotorRst
	
	
	Color...focus
	Display the status

	
	Return
	
	▲
	

	All Reset''
	
	
	"Annu"
	Cancel

	
	
	
	"Exec"
	Reset

	

XY Rst
	PAN/tilt
RESET
	
	"Annu"
	Cancel

	
	
	
	"Exec"
	Reset

	

EffecRst
	

Effect reset
	
	"Annu"
	Cancel

	
	
	
	"Exec"
	Reset

	"ExitMenu"
	
	
	▲
	Exit



9. [bookmark: _Toc494321532]DMX Channels
	MODE 1
	MODE 2
	DMX Value
	Description

	1
	1
	0－255
	Pan

	2
	*
	0－255
	Pan Fine

	3
	2
	0－255
	Tilt

	4
	*
	0－255
	Tilt Fine

	5
	3
	0－255
	Pan/Tilt speed

	6
	4
	
	Micro

	
	
	0－19
	Empty

	
	
	20－24
	Energy-saving mode（230W）

	
	
	25－129
	Empty

	
	
	130－139
	Lamp on by dmx

	
	
	140－149
	PAN/TILT reset

	
	
	150－159
	Empty

	
	
	160－169
	Small motors reset

	
	
	170－199
	empty

	
	
	200－209
	Whole unit reset

	
	
	210－229
	empty

	
	
	230－239
	Lamp off by dmx

	
	
	240－255
	empty

	7
	5
	
	Colors

	
	
	0－8
	white

	
	
	9－17
	Deep Red

	
	
	18－26
	Deep blue

	
	
	27－36
	Yellow

	
	
	37－45
	Green

	
	
	46－54
	Magenta

	
	
	55－63
	Azure

	
	
	64－72
	Red

	
	
	73－81
	Dark green

	
	
	82－90
	Amber

	
	
	91－100
	blue

	
	
	101－109
	orange

	
	
	110－118
	CTO

	
	
	119－127
	UV

	
	
	128－129
	white

	
	
	Positioning

	
	
	130－134
	Deep Red

	
	
	135－138
	Deep blue

	
	
	139－143
	Yellow

	
	
	144－147
	Green

	
	
	148－152
	Magenta

	
	
	153－157
	Azure

	
	
	158－161
	Red

	
	
	162－166
	Dark green

	
	
	167－171
	Amber

	
	
	172－176
	blue

	
	
	177－180
	orange

	
	
	181－185
	CTO

	
	
	186－189
	UV

	
	
	190－215
	Forwards rainbow ,speed down

	
	
	216－217
	No rotation

	
	
	
218-243
	Backwards rainbow, speed up

	
	
	244-255
	Random color

	8
	*
	
	empty

	9
	6
	
	empty

	
	7
	
	Static gobo

	


















10
	
	0－3
	empty

	
	
	4－9
	Gobo 1

	
	
	10－15
	Gobo 2

	
	
	16－21
	Gobo 3

	
	
	22－27
	Gobo 4

	
	
	28－33
	Gobo 5

	
	
	34－39
	Gobo 6

	
	
	40－45
	Gobo 7

	
	
	46－51
	Gobo 8

	
	
	52－57
	Gobo 9

	
	
	58－63
	Gobo 10

	
	
	64－69
	Small beam 1

	
	
	70－75
	Small beam 2

	
	
	76－87
	Small beam 3

	
	
	
	Gobo shaking from slow to fast

	
	
	88－95
	shaking

	
	
	96－103
	Gobo 2

	
	
	104－111
	Gobo 3

	
	
	112－119
	Gobo 4

	
	
	120－127
	Gobo 5

	
	
	128－135
	Gobo 6

	
	
	136－143
	Gobo 7

	
	
	144－151
	Gobo 8

	
	
	152－159
	Gobo 9

	
	
	160－167
	Gobo 10

	
	
	168－175
	Small beam 1

	
	
	176－183
	Small beam 2

	
	
	184－199
	Small beam 3

	
	
	200－255
	Static gobo run from slow to fast

	





11
	





8
	
	Rotate gobo

	
	
	0－8
	empty

	
	
	9－17
	Gobo 1

	
	
	18－26
	Gobo 2

	
	
	27－35
	Gobo 3

	
	
	36－44
	Gobo 4

	
	
	45－53
	Gobo 5

	
	
	54－62
	Gobo 6

	
	
	63－71
	Gobo 7

	
	
	72－80
	Gobo 8

	
	
	81－89
	Gobo 9

	
	
	
	Gobo shaking from slow to fast

	
	
	90－97
	Shaking ,from slow to fast

	
	
	98－106
	Gobo 2

	
	
	107－115
	Gobo 3

	
	
	116－124
	Gobo 4

	
	
	125－133
	Gobo 5

	
	
	134－142
	Gobo 6

	
	
	143－151
	Gobo 7

	
	
	152－160
	Gobo 8

	
	
	161－169
	Gobo 9

	
	
	171－179
	Gobo 9 not move

	
	
	180－217
	Run from fast to slow

	
	
	218－255
	Run from slow to fast

	




12
	




9
	
	Gobo rotation

	
	
	0－127
	index

	
	
	128－177
	Run from slow to fast in anti clockwise

	
	
	178－203
	stop

	
	
	204－255
	Run from fast to slow in clockwise

	13
	*
	0－255
	empty

	


14
	


10
	
	prism

	
	
	0－19
	empty

	
	
	20－75
	6 linear prism

	
	
	76－255
	8 facet prism

	




15
	




11
	
	Prism rotation

	
	
	0－127
	index

	
	
	128－191
	Run from fast to slow in clockwise

	
	
	192－194
	empty

	
	
	195－255
	Run from slow to fast in anti clockwise

	16
	12
	
	Frost

	
	
	0－64
	empty

	
	
	65－255
	linear frost

	17
	13
	
	zoom

	
	
	0－255
	Linear zoom

	18
	*
	0－255
	Zoom fine

	19
	14
	0－255
	focus

	20
	*
	0－255
	Zoom fine

	21
	*
	0－255
	empty

	22
	15
	
	strobe

	
	
	0－31
	Strobe close

	
	
	32－63
	No Strobe

	
	
	64－95
	Strobe from slow to fast

	
	
	96－127
	No Strobe

	
	
	128－143
	Fast to slow,slow close fast open

	
	
	144－159
	Slow to fast,fast open slow close

	
	
	160－191
	Strobe open

	
	
	192－223
	Random strobe from slow to fast

	
	
	224－255
	No strobe

	23
	16
	
	dimmer

	
	
	0－255
	Linear dimmer

	24
	*
	
	empty



10. [bookmark: _Toc494321533]Clear and maintenance 
[image: d9abb482aa491d1f059f48412cb8b219]Warning: Please make sure cut off the power before open the covers.
(Kind Remind: Non-Professional don’t do this)
1. Cut off the power supply, cool down the lamp and open the covers.
2. Using vacuum or pressure blows gently blow any dust and floating structures.
[bookmark: _Toc362697090][bookmark: _Toc362698470]
11. [bookmark: _Toc362697091][bookmark: _Toc362698471][bookmark: _Toc494321534]Contact:
Please check who is our dealer in your country at our website

www.kudux.com

or write direct to us by email:  office@kudux.com
WWW.KUDUX.COM	                         19
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